Beam Magnet Corrector/Kicker Assembly (metric)

Beam Line Mount (block comprises 2 diagonal halves)

 

# Magnet Coil (4 each)



**Notes:**

* All units of measurement are in millimeters except screw holes.
* Holes (in yellow) are threaded for size 10-32 x ½” Allen head screws.
* All materials must be non-magnetic.
* Winding wire diameter is around 0.35mm (measured by caliper)
* Winding OD is 52.31mm (measured by caliper)